Initializing help system before first use

# XSLP_BARCROSSOVERSTART, SLPBARCROSSOVERSTART

Description | Default crossover activation behaviour for barrier start
Type | Integer
Topic areas | SLP, Linearizations
Default value | 0
Note | When XSLP_BARLIMIT is set, XSLP_BARCROSSOVERSTART offers an overwrite control on when crossover is applied. A positive value indicates that crossover should be disabled in iterations smaller than XSLP_BARCROSSOVERSTART and should be enabled afterwards, or when stalling is detected as described in XSLP_BARSTARTOPS. A value of 0 indicates to respect the value of XPRS_CROSSOVER and only overwrite its value when stalling is detected. A value of -1 indicates to always rely on the value of XPRS_CROSSOVER.
Affects routines | XSLPmaxim, XSLPminim
See also | XSLP_BARLIMIT, XSLP_BARSTARTOPS, XSLP_BARSTALLINGLIMIT, XSLP_BARSTALLINGOBJLIMIT, XSLP_BARSTALLINGTOL
Category | Control

Parent Topic Integer control parameters

© 2001-2026 Fair Isaac Corporation. All rights reserved. This documentation is the property of Fair Isaac Corporation (“FICO”). Receipt or possession of this documentation does not convey rights to disclose, reproduce, make derivative works, use, or allow others to use it except solely for internal evaluation purposes to determine whether to purchase a license to the software described in this documentation, or as otherwise set forth in a written software license agreement between you and FICO (or a FICO affiliate). Use of this documentation and the software described in it must conform strictly to the foregoing permitted uses, and no other use is permitted.