Initializing help system before first use

# TUNERMAXTIME

Description | Tuner: The maximum time in seconds that the tuner will run before it terminates.
Type | Double
Topic areas | Tuner, Limits
Values |
0 | No time limit.
>0 | Stop the tuner after the given number of seconds.
Default value | 0
Note | This control changed type with Xpress Optimizer version 9.0 (from integer to double). It is strongly recommended to adapt all access calls to this control accordingly. This control only has an effect on the tuner.
Affects routines | XPRStune ( TUNE).
See also | TIMELIMIT.
Category | Control

Parent Topic Control Parameters

© 2001-2026 Fair Isaac Corporation. All rights reserved. This documentation is the property of Fair Isaac Corporation (“FICO”). Receipt or possession of this documentation does not convey rights to disclose, reproduce, make derivative works, use, or allow others to use it except solely for internal evaluation purposes to determine whether to purchase a license to the software described in this documentation, or as otherwise set forth in a written software license agreement between you and FICO (or a FICO affiliate). Use of this documentation and the software described in it must conform strictly to the foregoing permitted uses, and no other use is permitted.