Initializing help system before first use

# BARREGULARIZE

Description | This bit-vector control (see Section Bit-vector controls) determines how the barrier algorithm applies regularization on the KKT system.
Type | Integer
Topic areas | Barrier, Bit-vector
Values |
Bit | Meaning
0 | Standard regularization is turned on/off.
1 | Reduced regularization is turned on/off. This option reduces the perturbation effect of the standard regularization.
2 | Forces to keep dependent rows in the KKT system.
3 | Forces to preserve degenerate rows in the KKT system.
4 | Restrict regularization to infeasible iterates.
5 | Disable iterative regularizations.
6 | Apply iterative regularization more often.
Default value | -1
Note | If the value of the control is set to -1 (default) then the solver will automatically select the bits it deems most useful.
Affects routines | XPRSlpoptimize ( LPOPTIMIZE), XPRSmipoptimize ( MIPOPTIMIZE).
Category | Control

Parent Topic Control Parameters

© 2001-2026 Fair Isaac Corporation. All rights reserved. This documentation is the property of Fair Isaac Corporation (“FICO”). Receipt or possession of this documentation does not convey rights to disclose, reproduce, make derivative works, use, or allow others to use it except solely for internal evaluation purposes to determine whether to purchase a license to the software described in this documentation, or as otherwise set forth in a written software license agreement between you and FICO (or a FICO affiliate). Use of this documentation and the software described in it must conform strictly to the foregoing permitted uses, and no other use is permitted.